§192.16   Customer notification

The City of Dilley does not maintain the customer's buried piping.
If the customer's buried piping is not maintained, it may be subject to the potential hazards of corrosion and leakage.
(1) Buried gas piping should be—
(i) Periodically inspected for leaks;
(ii) Periodically inspected for corrosion if the piping is metallic; and
(iii) Repaired if any unsafe condition is discovered.
(2) When excavating near buried gas piping, the piping should be located in advance, and the excavation done by hand.
(3) The City (if applicable), plumbing contractors, and heating contractors can assist in locating, inspecting, and repairing the customer's buried piping.

